For a 1-radian step reference, the design criteria are given are the following.

* • Settling time less than 0.040 seconds
* • Overshoot less than 16%
* • No steady-state error, even in the presence of a step disturbance input